## Importing Projects from a Bld.Inf File

The command-line Symbian OS toolchain requires that projects are defined with these formats:

- Symbian OS-specific project file formats (bld.inf)
- Symbian OS executable files (.exe)

The primary purpose of bld.inf files is to group together closely associated projects, such as a GUI application and a engine DLL used by that application.

The Symbian OS plug-ins allow you to import projects defined with these formats into the workbench. This is useful if:

- You have existing projects defined using these formats and now wish to move to development in Carbide.c++.

- You need to keep the ability to build from the command line, for example in order to do automated builds, and so maintain the command line project files, but want to use Carbide.c++ for editing code and debugging.

### Projects for Symbian OS 9.3+

The latest versions of Symbian OS 9.3+ devkits include extensive use of PRJ_EXTENSIONS and PRJ_TESTEXTENSIONS. These top-level entries are extension makefile templates whose names are later filled in with target names, sources, and options. The intent is to make source editing easier and dependency checking possible during a build.

Currently if you import a bld.inf file but are not importing all of the components and one of these extensions are found:

- a warning appears at the top of the wizard page
- a warning is shown in the Carbide Project Settings property page
- if not building from the bld.inf, messages appear in the Console and Problems views

The reason being that individual extensions cannot be built from within Carbide, only the complete bld.inf.

#### To import from a bld.inf file

1. Click File > Import... to get a list of available import wizards
2. Select Symbian OS Bld.inf file and click Next to go to the Import Bld.inf page

3. Type the location of the bld.inf file to import, or browse to the file using the Browse button.

NOTE There will be two builders available in Carbide, one for SBSv1 (current version of Symbian Build System) and one for SBSv2 (newer version). The Builder option will only be displayed when a SBSv2 installation is detected.

SBSv2 only works with recent versions of Symbian OS9.5. Both SBSv1 and SBSv2 are GNU make based build systems. SBSv1 uses Perl to generate make files, while SBSv2 uses Python. Select the appropriate builder for your project.

When building for SBSv2, the builder will set EPOCROOT to the absolute path (including drive letter) to the kit for the active build configuration. It will also add the path to the sbs bin directory to the start of the PATH variable. This is derived from the SBS_HOME environment variable.

For SBSv2, all build configurations (platform/target), including the built-in platforms (WISNCW, ARMV5), are declared in xml files in the \sbs\lib\config directory. The Build Configurations selection page will display only those kits known to support SBSv2.

4. Click Next to select the recognized SDKs and Build Configurations to be created for this project

   The SDKs and Build Configurations shows a tree of the SDKs that are available to be used, and for each SDK, the type of build configurations that are available. You can select a single SDK if you are developing the program for just one version of a platform, or multiple SDKs if your program is to be built against multiple platforms or operating system versions.

   NOTE The platforms listed are dependent upon the filter settings in the Platform Filtering Preferences.

5. Click Next to select the mmp and extension make files

6. Click Next to enter the Project name and root directory

When creating a project, project files are created in the root directory. Carbide.c++ creates additional files for each project. They consist of:

- .project - an xml file that provides a project description
- .cproject - an xml file that provides additional project information
- .settings folder - contains files that provide build configuration and preference settings

The root directory is a path to the root of your project. All necessary tool components, developer libraries, and information about the SDK are stored in subdirectories under this root. The whole path leading to the SDK root directory must be declared to the Windows system via the Environment Variables settings. The variable name is EPOCROOT and the variable value is the full path where a Symbian OS SDK is installed in the Windows system.

The root directory should contain all project related files that you want to work with in Carbide. The default directory is calculated by parsing the bld.inf file and mmp file(s).

7. Click Finish to import the project

   The wizard creates the project in the C/C++ Projects view, where it can be built and edited as normal. If the wizard is unable to read the project files, then the page describes the error that occurred. If an error occurs, you must fix the project file, and then re-import the bld.inf.

##### Related concepts

- Projects
- Project Resources

##### Related tasks

- Creating Projects
- Building Projects
- Importing a Symbian Executable

##### Related references

- Platform Filtering Preferences
- Project Directories
- Project Preferences
- Project Types