## Stop Mode On-Device Debugging Preconditions

Before conducting a Stop Mode On-Device debug session the following preconditions should be met.

#### Verifying On-device Debugging Preconditions

- Install ActiveState PERL. You can download a copy of Perl at www.ActiveState.com.
- Install the GCCE or RVCT 2.2 or greater compiler (not included with Carbide.c++).
- Install the TechView Devkit
- Install Board Support Package (BSP) for your target board
- Install JTAG software and drivers for Trace32 support
- Connect JTAG interface between PC and hardware
- Verify that your SDK or customer kit is recognized in the SDK preferences panel.
- Build your ROM Image

##### Related Tasks

- Symbian OS Trace32 Support