#<bsf>#

# This BSF file is to support building for ARMV6 architecture ABIV2 mode. The options specified here are same as for 
# ARMV5_ABIV2 except the --cpu 6 option in INVARIANT_OPTIONS. This specifies to compiler to compile for generic ARMV6. 
# If any other specific options are required such as --cpu ARM1136J-S, etc, then it can be done 
# via a different BSF file.

# ARMV6_ABIV2 platform will be supported as an intermediate step before the migration to ABIv2. Once ARMV5 platform 
# switches to ABIv2 mode, ARMV6 platform also switches to ABIv2 and ARMV6_ABIV2 will be deprecated.

# NOTE: The compiler options specified here disable the unaligned memory access.

CUSTOMIZES ARMV5_ABIV2

INVARIANT_OPTIONS --cpu 6 --enum_is_int -Ono_known_library --fpmode ieee_no_fenv --export_all_vtbl --no_vfe --apcs /inter --memaccess -UL41
