# Copyright (c) 2009-2010 Nokia Corporation and/or its subsidiary(-ies).
# All rights reserved.
# This component and the accompanying materials are made available
# under the terms of the License "Eclipse Public License v1.0"
# which accompanies this distribution, and is available
# at the URL "http://www.eclipse.org/legal/epl-v10.html".
#
# Initial Contributors:
# Nokia Corporation - initial contribution.
#
# Contributors:
#
# Description:
#

# Bluetooth HCI Commands to be generated
# Syntax is documented below. ("[]" brackets are used for grouping with regexp wildcards, and wildcard operators will only directly follow a ']')
#
# COMMAND_NAME(COMMAND_CREDITS,EXPECTS_COMMAND_STATUS,EXPECTS_COMMAND_COMPLETE[,Match,MATCHING_EVENT_NAME,CONCLUDES_COMMAND,CONTINUE_MATCHING[,MATCH_OPERANDS]*]*): COMMAND_PARAMETERS
#
# Variables:
# COMMAND_NAME = The name of the command for which a class will be generated.
# COMMAND_CREDITS = The number of "command credits" this command consumes when sent to a controller.
# EXPECTS_COMMAND_STATUS = Boolean specifying whether the command expects a command status event from the controller in response.
# EXPECTS_COMMAND_COMPLETE = Boolean specifying whether the command expects a command complete event from the controller.
# MATCHING_EVENT_NAME = The name of an event that will be "matched" with this command
# CONCLUDES_COMMAND = Boolean specifying whether the matched event represents the conclusion of the request made by the command.
# CONTINUE_MATCHING = Boolean specifying whether the command queue should continue trying to match the event with other sent commands.
# MATCH_OPERANDS = Used to perform the match on more than just the event opcode.
#
# COMMAND_PARAMETERS = [COMMAND_PARAMETER]? [,COMMAND_BLOCK_PARAM]*
# COMMAND_PARAMETER = PARAMETER_NAME (PARAMETER_SIZE)
# COMMAND_BLOCK_PARAM = COMMAND_PARAMETER [* PARAMETER_NAME]
# The parameters to the command are typically just a name and a size.  If the parameters feature an array (e.g. WriteStoredLinkKey)
# then the '*' can be used to make the construct with the appropriate multiplicity.
#
#
##### 7.1 Link Control Commands
#
Inquiry(1,True,False,Match,InquiryResultEvent,False,False,Match,InquiryResultwithRSSIEvent,False,False,Match,ExtendedInquiryResultEvent,False,False,Match,InquiryCompleteEvent,True,False,Match,CommandCompleteEvent,True,True,CommandOpcode_KInquiryCancelOpcode): LAP (3) InquiryLength(1) NumResponses(1)
InquiryCancel(1,False,True,Match,CommandCompleteEvent,True,True,CommandOpcode_KInquiryCancelOpcode):
PeriodicInquiryMode(1,False,True): MaxPeriodLength (2), MinPeriodLength (2), LAP (3), InquiryLength (1), NumResponses (1)
ExitPeriodicInquiryMode(1,False,True):
CreateACLConnection(1,True,False,Match,ConnectionCompleteEvent,True,False,BDADDR): BDADDR (6), PacketType (2), PageScanRepetitionMode (1), Reserved (1), ClockOffset (2), AllowRoleSwitch (1)
Disconnect(1,True,False,Match,DisconnectionCompleteEvent,True,False,ConnectionHandle): ConnectionHandle (2), Reason (1)
CreateConnectionCancel(1,False,True): BDADDR (6)
AcceptConnectionRequest(1,True,False,Match,ConnectionCompleteEvent,True,False,BDADDR): BDADDR (6), Role (1)
RejectConnectionRequest(1,True,False,Match,ConnectionCompleteEvent,True,False,BDADDR): BDADDR (6), Reason (1)
LinkKeyRequestReply(1,False,True): BDADDR (6), LinkKey (16)
LinkKeyRequestReplyNegative(1,False,True): BDADDR (6)
PINCodeRequestReply(1,False,True): BDADDR (6), PINCodeLength (1), PINCode (16)
PINCodeRequestReplyNegative(1,False,True): BDADDR (6)
ChangeConnectionPacketType(1,True,False,Match,ConnectionPacketTypeChangedEvent,True,False): ConnectionHandle (2), PacketType (2)
AuthenticationRequested(1,True,False,Match,AuthenticationCompleteEvent,True,False): ConnectionHandle (2)
SetConnectionEncryption(1,True,False,Match,EncryptionChangeEvent,True,False): ConnectionHandle (2), EncryptionEnable (1)
ChangeLinkKey(1,True,False,Match,LinkKeyNotificationEvent,False,False,Match,ChangeLinkKeyEvent,True,False): ConnectionHandle (2)
MasterLinkKey(1,True,False,Match,MasterLinkKeyEvent,True,False): KeyFlag (1)
RemoteNameRequest(1,True,False,Match,RemoteNameReqCompleteEvent,True,False,Match,RemoteHostSupportedFeaturesNotificationEvent,False,False): BDADDR (6), PageScanRepetitionMode (1), Reserved (1), ClockOffset (2)
RemoteNameRequestCancel(1,False,True): BDADDR (6)
ReadRemoteSupportedFeatures(1,True,False,Match,ReadRemSuppFeatCompleteEvent,True,False): ConnectionHandle (2)
ReadRemoteExtendedFeatures(1,True,False,Match,ReadRemoteExtendedFeaturesCompleteEvent,True,False): ConnectionHandle (2), PageNumber (1)
ReadRemoteVersionInfo(1,True,False,Match,ReadRemVerInfoCompleteEvent,True,False): ConnectionHandle (2)
ReadClockOffset(1,True,False,Match,ReadClockOffsetEvent,True,False): ConnectionHandle (2)
ReadLMPHandle(1,False,True): ConnectionHandle (2)
SetupSynchronousConnection(1,True,False,Match,SynchronousConnectionCompleteEvent,True,False,BDADDR,Match,SynchronousConnectionChangedEvent,True,False): ConnectionHandle (2), TransmitBandwidth (4), ReceiveBandwidth (4), MaxLatency (2), VoiceSetting (2), RetransmissionEffort (1), PacketType (2), @BDADDR (6)
AcceptSynchronousConnectionRequest(1,True,False,Match,SynchronousConnectionCompleteEvent,True,False,BDADDR): BDADDR (6), TransmitBandwidth (4), ReceiveBandwidth (4), MaxLatency (2),  ContentFormat (2), RetransmissionEffort (1), PacketType (2)
RejectSynchronousConnectionRequest(1,True,False,Match,SynchronousConnectionCompleteEvent,True,False,BDADDR): BDADDR (6), Reason (1)
IOCapabilityRequestReply(1,False,True,Match,IOCapabilityResponseEvent,False,False,Match,RemoteOOBDataRequestEvent,False,False): BDADDR (6), IOCapability (1), OOBDataPresent (1), AuthenticationRequirements (1)
UserConfirmationRequestReply(1,False,True): BDADDR (6)
UserConfirmationRequestNegativeReply(1,False,True): BDADDR (6)
UserPasskeyRequestReply(1,False,True): BDADDR (6), NumericValue (4)
UserPasskeyRequestNegativeReply(1,False,True): BDADDR (6)
RemoteOOBDataRequestReply(1,False,True): BDADDR (6), OOBDataC (16), OOBDataR (16)
RemoteOOBDataRequestNegativeReply(1,False,True): BDADDR (6)
IOCapabilityRequestNegativeReply(1,False,True): BDADDR (6), Reason (1)
#
##### 7.2 Link Policy Commands
#
HoldMode(1,True,False,Match,ModeChangeEvent,True,False,ConnectionHandle): ConnectionHandle (2), HoldModeMaxInterval (2), HoldModeMinInterval (2)
SniffMode(1,True,False,Match,ModeChangeEvent,True,False,ConnectionHandle): ConnectionHandle (2), SniffMaxInterval (2), SniffMinInterval (2), SniffAttempt (2), SniffTimeout (2)
ExitSniffMode(1,True,False,Match,ModeChangeEvent,True,False,ConnectionHandle): ConnectionHandle (2)
ParkMode(1,True,False,Match,ModeChangeEvent,True,False,ConnectionHandle): ConnectionHandle (2), BeaconMaxInterval (2), BeaconMinInterval (2)
ExitParkMode(1,True,False,Match,ModeChangeEvent,True,False,ConnectionHandle): ConnectionHandle (2)
QOSSetup(1,True,False,Match,QOSSetupCompleteEvent,True,False): ConnectionHandle (2), Flags (1), ServiceType (1), TokenRate (4), PeakBandwidth (4), Latency (4), DelayVariation (4)
RoleDiscovery(1,False,True): ConnectionHandle (2)
SwitchRole(1,True,False,Match,RoleChangeEvent,True,False,BDADDR): BDADDR (6), Role (1)
ReadLinkPolicySettings(1,False,True): ConnectionHandle (2)
WriteLinkPolicySettings(1,False,True): ConnectionHandle (2), LinkPolicySettings (2)
ReadDefaultLinkPolicySettings(1,False,True):
WriteDefaultLinkPolicySettings(1,False,True): DefaultLinkPolicySettings (2)
FlowSpecification(1,True,False,Match,FlowSpecificationCompleteEvent,True,False): ConnectionHandle (2), Flags (1), FlowDirection (1), ServiceType (1), TokenRate (4), TokenBucketSize (4), PeakBandwidth (4), AccessLatency (4)
### SniffSubrating command would match with a sniff subrating event, however if not in sniff mode then the
### sniff subrating event will not be generated until sniff mode is entered, so we cannot match as we need to
### conclude the sniff subrating command upon the receipt of the command complete event. As it appears that 
### we would expect the sniff subrating event after the complete matching to the sniff subrating event 
### is pointless. 
SniffSubrating(1,False,True): ConnectionHandle (2), MaximumLatency (2), MinimumRemoteTimeout (2), MinimumLocalTimeout (2)
#
##### 7.3 Controller & Baseband Commands
#
SetEventMask(1,False,True): EventMask (8)
Reset(1,False,True):
SetEventFilter(1,False,True): FilterType (1), FilterConditionType (1), Condition (7)
Flush(1,False,True,Match,FlushOccurredEvent,False,False): ConnectionHandle (2)
ReadPINType(1,False,True):
WritePINType(1,False,True): PINType (1)
CreateNewUnitKey(1,False,True):
ReadStoredLinkKey(1,False,True,Match,ReturnLinkKeysEvent,False,False): BDADDR (6), ReadAllFlag (1)
WriteStoredLinkKey(1,False,True): NumKeysToWrite (1), BDADDR (6) * NumKeysToWrite, LinkKey (16) * NumKeysToWrite
DeleteStoredLinkKey(1,False,True): BDADDR (6), DeleteAllFlag (1)
WriteLocalName(1,False,True): LocalName (248)
ReadLocalName(1,False,True):
ReadConnectionAcceptTimeout(1,False,True):
WriteConnectionAcceptTimeout(1,False,True): ConnAcceptTimeout (2)
ReadPageTimeout(1,False,True):
WritePageTimeout(1,False,True): PageTimeout (2)
ReadScanEnable(1,False,True):
WriteScanEnable(1,False,True): ScanEnable (1)
ReadPageScanActivity(1,False,True):
WritePageScanActivity(1,False,True): PageScanInterval (2), PageScanWindow (2)
ReadInquiryScanActivity(1,False,True):
WriteInquiryScanActivity(1,False,True): InquiryScanInterval (2), InquiryScanWindow (2)
ReadAuthenticationEnable(1,False,True):
WriteAuthenticationEnable(1,False,True): AuthenticationEnable (1)
ReadClassOfDevice(1,False,True):
WriteClassOfDevice(1,False,True): ClassOfDevice (3)
ReadVoiceSetting(1,False,True):
WriteVoiceSetting(1,False,True): VoiceSetting (2)
ReadAutomaticFlushTimeout(1,False,True): ConnectionHandle (2)
WriteAutomaticFlushTimeout(1,False,True): ConnectionHandle (2), FlushTimeout (2)
ReadNumBroadcastRetransmissions(1,False,True):
WriteNumBroadcastRetransmissions(1,False,True): NumBroadcastRetransmissions (1)
ReadHoldModeActivity(1,False,True):
WriteHoldModeActivity(1,False,True): HoldModeActivity (1)
ReadTransmitPowerLevel(1,False,True): ConnectionHandle (2), Type (1)
ReadSynchronousFlowControlEnable(1,False,True):
WriteSynchronousFlowControlEnable(1,False,True): SynchronousFlowControlEnable (1)
SetControllerToHostFlowControl(1,False,True): FlowControlEnable (1)
HostBufferSize(1,False,True): HostACLDataPacketLength (2), HostSynchronousDataPacketLength (1), HostTotalNumACLDataPackets (2), HostTotalNumSynchronousDataPackets (2)
HostNumberOfCompletedPackets(0,False,False): NumberOfHandles (1), ConnectionHandle (2) * NumberOfHandles, HostNumOfCompletedPackets (2) * NumberOfHandles
ReadLinkSupervisionTimeout(1,False,True): ConnectionHandle (2)
WriteLinkSupervisionTimeout(1,False,True): ConnectionHandle (2), LinkSupervisionTimeout (2)
ReadNumberOfSupportedIAC(1,False,True):
ReadCurrentIACLAP(1,False,True):
WriteCurrentIACLAP(1,False,True): NumCurrentIAC (1), IACLAP (3) * NumCurrentIAC
SetAFHHostChannelClassification(1,False,True): AFHHostChannelClassification (10)
ReadInquiryScanType(1,False,True):
WriteInquiryScanType(1,False,True): ScanType (1)
ReadInquiryMode(1,False,True):
WriteInquiryMode(1,False,True): InquiryMode (1)
ReadPageScanType(1,False,True):
WritePageScanType(1,False,True): PageScanType (1)
ReadAFHChannelAssessmentMode(1,False,True):
WriteAFHChannelAssessmentMode(1,False,True): AFHChannelAssessmentMode (1)
ReadExtendedInquiryResponse(1,False,True):
WriteExtendedInquiryResponse(1,False,True): FECRequired (1), ExtendedInquiryResponse (240) 
RefreshEncryptionKey(1,True,False,Match,EncryptionKeyRefreshCompleteEvent,True,False,ConnectionHandle): ConnectionHandle (2)
ReadSimplePairingMode(1,False,True):
WriteSimplePairingMode(1,False,True): SimplePairingMode (1)
ReadLocalOOBData(1,False,True):
ReadInquiryResponseTransmitPowerLevel(1,False,True):
WriteInquiryResponseTransmitPowerLevel(1,False,True): TxPowerLevel (1)
SendKeypressNotification(1,False,True): BDADDR (6), NotificationType (1)
ReadDefaultErroneousDataReporting(1,False,True):
WriteDefaultErroneousDataReporting(1,False,True): ErroneousDataReporting (1)
EnhancedFlush(1,True,False,Match,EnhancedFlushCompleteEvent,True,False,ConnectionHandle): ConnectionHandle (2), PacketType (1)
#
##### 7.4 Informational Parameters
#
ReadLocalVersionInfo(1,False,True):
ReadLocalSupportedCommands(1,False,True):
ReadLocalSupportedFeatures(1,False,True):
ReadLocalExtendedFeatures(1,False,True): PageNumber (1)
ReadBufferSize(1,False,True):
ReadBdaddr(1,False,True):
#
##### 7.5 Status Parameters
#
ReadFailedContactCounter(1,False,True): ConnectionHandle (2)
ResetFailedContactCounter(1,False,True): ConnectionHandle (2)
ReadLinkQuality(1,False,True): ConnectionHandle (2)
ReadRSSI(1,False,True): ConnectionHandle (2)
ReadAFHChannelMap(1,False,True): ConnectionHandle (2)
ReadClock(1,False,True): ConnectionHandle (2), WhichClock (1)
#
##### 7.6 Testing Commands
#
ReadLoopbackMode(1,False,True):
WriteLoopbackMode(1,False,True): LoopbackMode (1)
EnableDeviceUnderTestMode(1,False,True):
WriteSimplePairingDebugMode(1,False,True): SimplePairingDebugMode (1)
#
#### Appendix A: Deprecated Commands, Events and Configuration Parameters
#
ReadPageScanPeriod(1,False,True):
WritePageScanPeriod(1,False,True): PageScanPeriodMode (1)
AddSCOConnection(1,True,False,Match,ConnectionCompleteEvent,True,False,BDADDR): ConnectionHandle (2), PacketType (2), @BDADDR (6)
ReadEncryptionMode(1,False,True):
WriteEncryptionMode(1,False,True): EncryptionMode (1)
