{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["PDU DB","SUBMIT","DELIVER"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PDU DB","index":0,"n_rows":7,"n_cols":2,"rows_kept":7,"flags":["formulas_cached_only"]}
[]
[]
[null,"This is a database of PDUs as a resource for testing.  It is called PDU DB"]
[]
[null,"PDUs stored here can easily be assembled from the clearly marked fields.  Some PDUs can be used as is; Some will require a little bit of engineering."]
[]
[null,"PDUs can be added easily"]

{"sheet":"SUBMIT","index":1,"n_rows":28,"n_cols":15,"rows_kept":28,"flags":["formulas_cached_only"]}
[]
[]
[null,"Number","Description","Message","PDU","Header","MR","TelNumber","PID","DCS","VP","UDL","UDHL","UDH","UD"]
[]
[]
[null,1,"Single PDU 8bit message","test message, 8bits, length 30","15000C915348801455820004A71E74657374206D6573736167652C2038626974732C206C656E677468203330",15,"00","0C91534880145582","00","04","A7","1E",null,null,"74657374206D6573736167652C2038626974732C206C656E677468203330"]
[]
[null,2,"1st PDU of 3 PDU 8bit message NO class","This is test message ONE","15000C915348801455820004A71E0003000301546869732069732074657374206D657373616765204F6E65",15,"00","0C91534880145582","00","04","A7","1E","05","0003000301","546869732069732074657374206D657373616765204F4E45"]
[]
[null,3,"1st PDU of 3 PDU 8bit message NO class","This is test message TWO","15000C915348801455820004A718546869732069732074657374206D6573736167652054574F",15,"00","0C91534880145582","00","04","A7","1E","05","0003010301","546869732069732074657374206D6573736167652054574F"]
[]
[null,4,"1st PDU of 3 PDU 8bit message NO class","This is test message THREE","15000C915348801455820004A71A546869732069732074657374206D657373616765205448524540",15,"00","0C91534880145582","00","04","A7",20,"05","0003020301","546869732069732074657374206D657373616765205448524540"]
[]
[null,5,"1st PDU of 3 PDU 8bit message NO class","This is test message FOUR","15000C915348801455820004A719546869732069732074657374206D65737361676520464F5552",15,"00","0C91534880145582","00","04","A7","1F","05","0003030301","546869732069732074657374206D65737361676520464F5552"]
[]
[null,6,"1st PDU of 3 PDU 8bit message NO class","This is test message FIVE","15000C915348801455820004A719546869732069732074657374206D6573736167652046495645",15,"00","0C91534880145582","00","04","A7","1F","05","0003040301","546869732069732074657374206D6573736167652046495645"]
[]
[null,7,"1st PDU of 3 PDU 8bit message NO class","This is test message SIX","15000C915348801455820004A718546869732069732074657374206D65737361676520534958",15,"00","0C91534880145582","00","04","A7","1E","05","0003050301","546869732069732074657374206D65737361676520534958"]
[]
[null,8,"1st PDU of 3 PDU 8bit message NO class","This is test message SEVEN","15000C915348801455820004A71A546869732069732074657374206D65737361676520534556454E",15,"00","0C91534880145582","00","04","A7",20,"05","0003060301","546869732069732074657374206D65737361676520534556454E"]
[]
[null,9,"1st PDU of 3 PDU 8bit message NO class","This is test message EIGHT","15000C915348801455820004A71A546869732069732074657374206D657373616765204549474854",15,"00","0C91534880145582","00","04","A7",20,"05","0003070301","546869732069732074657374206D657373616765204549474854"]
[]
[null,10,"1st PDU of 3 PDU 8bit message NO class","This is test message NINE","15000C915348801455820004A719546869732069732074657374206D657373616765204E494E45",15,"00","0C91534880145582","00","04","A7","1F","05","0003080301","546869732069732074657374206D657373616765204E494E45"]
[]
[null,11,"1st PDU of 3 PDU 8bit message NO class","This is test message TEN","15000C915348801455820004A718546869732069732074657374206D6573736167652054454E",15,"00","0C91534880145582","00","04","A7","1E","05","0003090301","546869732069732074657374206D6573736167652054454E"]
[]
[null,12,"1st PDU of 3 PDU 8bit message NO class","This is test message ELEVEN","15000C915348801455820004A71B546869732069732074657374206D65737361676520454C4556454E",15,"00","0C91534880145582","00","04","A7",21,"05","00030A0301","546869732069732074657374206D65737361676520454C4556454E"]

{"sheet":"DELIVER","index":2,"n_rows":34,"n_cols":14,"rows_kept":34,"flags":["formulas_cached_only"]}
[]
[]
[null,"Number","Description","Message","PDU","Header","Originating ","PID","DCS","SCTS","UDL","UDHL","UDH","UD"]
[{"$nulls":6},"Address"]
[]
[null,1,"Single PDU 8bit message","test message, 8bits, length 30","240C915348801455820014108071417314801E74657374206D6573736167652C2038626974732C206C656E677468203330",24,"0C91534880145582","00",14,"10807141731480","1E",null,null,"74657374206D6573736167652C2038626974732C206C656E677468203330"]
[]
[null,2,"1st PDU of 3 PDU 8bit message class 0","This is test message ONE","440C915348801455820014108071417314801E050003000301546869732069732074657374206D657373616765204F4E45",44,"0C91534880145582","00",14,"10807141731480","1E","05","0003000301","546869732069732074657374206D657373616765204F4E45"]
[]
[null,3,"1st PDU of 3 PDU 8bit message class 0","This is test message TWO","440C915348801455820014108071417314801E050003010301546869732069732074657374206D6573736167652054574F",44,"0C91534880145582","00",14,"10807141731480","1E","05","0003010301","546869732069732074657374206D6573736167652054574F"]
[]
[null,4,"1st PDU of 3 PDU 8bit message class 0","This is test message THREE","440C9153488014558200141080714173148020050003020301546869732069732074657374206D657373616765205448524540",44,"0C91534880145582","00",14,"10807141731480",20,"05","0003020301","546869732069732074657374206D657373616765205448524540"]
[]
[null,5,"1st PDU of 3 PDU 8bit message class 0","This is test message FOUR","440C915348801455820014108071417314801F050003030301546869732069732074657374206D65737361676520464F5552",44,"0C91534880145582","00",14,"10807141731480","1F","05","0003030301","546869732069732074657374206D65737361676520464F5552"]
[]
[null,6,"1st PDU of 3 PDU 8bit message class 0","This is test message FIVE","440C915348801455820014108071417314801F050003040301546869732069732074657374206D6573736167652046495645",44,"0C91534880145582","00",14,"10807141731480","1F","05","0003040301","546869732069732074657374206D6573736167652046495645"]
[]
[null,7,"1st PDU of 3 PDU 8bit message class 0","This is test message SIX","440C915348801455820014108071417314801E050003050301546869732069732074657374206D65737361676520534958",44,"0C91534880145582","00",14,"10807141731480","1E","05","0003050301","546869732069732074657374206D65737361676520534958"]
[]
[null,8,"1st PDU of 3 PDU 8bit message class 0","This is test message SEVEN","440C9153488014558200141080714173148020050003060301546869732069732074657374206D65737361676520534556454E",44,"0C91534880145582","00",14,"10807141731480",20,"05","0003060301","546869732069732074657374206D65737361676520534556454E"]
[]
[null,9,"1st PDU of 3 PDU 8bit message class 0","This is test message EIGHT","440C9153488014558241141080714173148020050003070301546869732069732074657374206D657373616765204549474854",44,"0C91534880145582","00",14,"10807141731480",20,"05","0003070301","546869732069732074657374206D657373616765204549474854"]
[]
[null,10,"1st PDU of 3 PDU 8bit message class 0","This is test message NINE","440C915348801455824114108071417314801F050003080301546869732069732074657374206D657373616765204E494E45",44,"0C91534880145582","00",14,"10807141731480","1F","05","0003080301","546869732069732074657374206D657373616765204E494E45"]
[]
[null,11,"1st PDU of 3 PDU 8bit message class 0","This is test message TEN","440C915348801455824114108071417314801E050003090301546869732069732074657374206D6573736167652054454E",44,"0C91534880145582","00",14,"10807141731480","1E","05","0003090301","546869732069732074657374206D6573736167652054454E"]
[]
[null,12,"1st PDU of 3 PDU 8bit message class 0","This is test message ELEVEN","440C91534880145582411410807141731480210500030A0301546869732069732074657374206D65737361676520454C4556454E",44,"0C91534880145582","00",14,"10807141731480",21,"05","00030A0301","546869732069732074657374206D65737361676520454C4556454E"]
[]
[null,13,"1st PDU of 3 PDU 8bit message class 0","I am the FIRST PDU ","440C9153488014558200F410807141731480190500030B03014920616D207468652046495253542050445520",44,"0C91534880145582","00","F4","10807141731480",19,"05","00030B0301","4920616D207468652046495253542050445520"]
[]
[null,14,"2nd PDU of a 3 PDU 8bit message class0","I am the SECOND PDU ","440C9153488014558200F4108071417314801A0500030B03024920616D20746865205345434F4E442050445520",44,"0C91534880145582","00","F4","10807141731480","1A","05","00030B0302","4920616D20746865205345434F4E442050445520"]
[]
[null,15,"3rd PDU of a 3 PDU 8bit message class0","I am the THIRD PDU","440C9153488014558200F410807141731480180500030B03034920616D2074686520544849524420504455",44,"0C91534880145582","00","F4","10807141731480",18,"05","00030B0303","4920616D2074686520544849524420504455"]